[bookmark: _ptjoz7z9qjkz]Site Manager Checklist
1. Create Clean/Dirty line (remember you can always make bigger but not smaller)
2. Control the flow of traffic, people and vehicles
3. Visitor logs, everyone on site checks in and out Daily
4. No one crosses line without proper PPE (Tyvek, boot covers, gloves, hairnet, mask)
5. Assist with supplies and requests at the line
6. Upon leaving, observe doffing procedures and make sure properly disposed of
7. Before exiting, everyone must be disinfected and hand sanitized
8. Be observant of surroundings
9. Work with Logistics on any needed supplies
10. Any issues or concerns should be reported to Operations Section Chief ASAP
[image: A detailed diagram illustrating a hazardous site layout divided into three color-coded zones: the Hot Zone or Exclusion Zone (EZ) at the top, separated by Control Access Points; the middle yellow Warm Zone or Contamination Reduction Zone (CRZ), featuring a striped diagonal Decontamination Corridor with a transport vehicle inside; and the green Cold Zone or Support Zone (SZ) at the bottom.]
[bookmark: _yfd27fehclk7]Supplies
	Category 1
	Category 2
	Category 3

	Tyvek
	Virkon
	Signage

	Gloves
	Sprayer
	Flashlight

	Boot Covers
	Tubs/Pans
	Important Phone numbers

	Hairnets
	Scrub Brush
	Trash bags/Can

	Masks
	Visitor Logs
	Dumpster

	Safety Glasses
	Caution Tape
	Pens & Markers

	Duct Tape
	Cones
	Bottled Water

	Lysol
	Tent??
	Table

	Hand Sanitizer
	Misc. Tools
	Chair
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